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USB&WiFi Handheld Ultrsound Scanner 
(For Cosmetic Facial Plastic Surgery)
Model: Airscan Faci6
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Features：
- It used for Mapping & Injection, evaluating filler.
- Lighter and smaller (only 155g) easy to carry.
- Full waterproof design, IPX8 convenient for sterilization.
-USB&WiFi two connections
-Support working while charging
-Free App, no membership fee, support IOS/Android/Windows.
-Built-in cooling coating
-Software feature:
√Support Dicom
√ Report edit/print
√ Free app & updates, Unlimited users
√ Horizontal&Vercal Screen display
√ Dual-screen display in different modes

Specification:
	Index 
	Contents

	Model Name
	Airscan Faci6

	Type
	USB&WiFi Handheld Ultrsound Scanner 

	Application
	Cosmetic Facial Plastic Surgery

	Frequency
	16-20Mhz

	Scan Depth
	10-40mm

	Elements
	192

	Display Mode
	B.B+M.Color.PW. PDI

	Channe
	6

	Image Management
	JPEG, MP4, Dicom ,Save&Share,image/video/report

	Connection
	USB&WiFi

	System Support
	Android. IOS. Windows

	Devic Support
	Android :Tablet/Phone/TV
IOS :Ipad/iPhone (only WiFi)
Windows PC

	Battery Capacity
	2200 mAh

	Battery Working time
	3h, 48h Ultra-long standb

	Recharge time
	2~3h by
USB cable or wireless chargin

	Adjustable Parameters
	B/Color GN(Gain)
D(Depth)
ENH(Enhancement)
DR(Dynamic Range)
H(harmonic)
Focus
8 TGC
Mid-Line
An note
Biopsy Puncture
Page Left/Right Up/Down

	Dimensions
	155x65x25mm

	Weight
	155g
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Zygomaticorbital artery near the eye
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One stop Medical Solution Provider


POWER BY: 
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LANNX Bio&Med Co.,Ltd
Website: www.lannx.net
E-Mail: sale@lannx.net

LANNX Bio&Med Co.,Ltd                                                        www.lannx.net
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