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GYD10J型振动压路机
GYD10J DOUBLE DRUM VIBRATORY ROLLER
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	规格型号：GYD10J型振动压路机

	Model：GYD10J Double drum vibratory roller

	一、适用范围 Application
GYD10J型振动压路机适用于公路维修、市政、乡村道路、停车场、体育场和其他工业场地等一般路面基础和沥青面层的压实。
GYD10J vibratory roller is suitable for the compaction of general pavement foundation and asphalt surface layer such as road maintenance, municipal, rural roads, parking lots, stadiums and other industrial sites.
二、性能特点
1、机械驱动，三档行驶速度；
Mechanical drive, three speeds.
2、液压后轮振动，单频单幅，电控起振，激振力大，压实效率高；
Hydraulic rear wheel vibration, single-frequency single amplitude, electronically controlled starting vibration, large excitation force, high compaction efficiency.
3、液压转向，铰接式车架，操作轻便灵活；
Hydraulic steering, articulated frame, light and flexible operation.
4、配置防腐大容量洒水箱，电控压力喷洒水系统；
Equipped with anti-corrosive large-capacity sprinkler tank, electronically controlled pressure sprinkler system.
5、操纵台及驾驶室可大角度翻起，维护保养触手可得；
The console and cab can be tilted up at a wide angle, so maintenance is within easy reach.
6、双方向盘和操纵设计，便于操作者观察边缘压实；
Dual steering wheel and maneuvering design for easy operator observation of edge compaction.
7、液压元件采用知名品牌，性能可靠；
Hydraulic components adopt well-known brands, reliable performance.
8、标配驾驶室，可选配棚架。
Standard cab with optional canopy.

	二、主要技术参数 Main parameters

	1、工作质量 Operating weight
	10000 kg

	2、振动轮直径 Vibratory drum diameter
	1200 mm

	3、压实宽度 Vibratory drum width
	1700 mm

	4、静线载荷 Static line pressure
	317 N/cm

	5、行驶速度 Travelling speed
	Ⅰ 2.5  Ⅱ 5.0  Ⅲ 8.5 km/h

	6、爬坡能力 Grade ability
	20%

	7、振动频率 Vibratory frequency
	45 Hz

	8、理论振幅 Vibratory amplitude
	0.45/0.7 mm

	9、激振力 Centrifugal force
	85/100 kN

	10、最小离地间隙 Min. Ground clearance
	280 mm 

	11、最小转弯半径 Min. turning radius
	6500 mm

	12、轴距 Wheel base
	3220 mm

	13、洒水箱容积 Water tank
	200x2 L

	14、燃油箱容积 Fuel tank
	150 L

	15、液压油箱 Hydraulic oil tank
	190 L

	15、外形尺寸（长×宽×高）   Dimension       
	4900×2090×2800 mm

	16、发动机 Engine
	康明斯 CUMMINS

	柴油机型号 Model
	4BT3.9-C100

	型式 Type
	4 cylinder in-line，4 stroke，water cooled

	标定功率 Rated power
	75 kW

	标定转速 Rated speed
	2400 r/min


主要配置说明 Main configuration
	序号
S/N

	名 称
ITEM
	规格型号
MODEL
	数量
NO.
	制造商
MANUFACTURER

	1
	柴油机
Engine
	4BT3.9-C100
	1
	东风康明斯
CUMMINS

	2
	振动泵
Vibratory pump
	P3100（15-14）
	1
	泊姆克
PERMCO

	3
	振动马达
Vibratory motor
	M124（20-54）
	1
	泊姆克
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